Install process for cris architecture.
______________________________________

http://www.axis.com for more info about the ETRAX 100LX module.

The latest osip release tested with cris was 0.8.7.

$> mkdir bld-osip
$> cd bld-osip

$> CC="gcc_cris -mlinux -isystem 
    /ldata/axis/cris-source/axis/devboard_lx/os/linux/include \
   -I/ldata/axis/cris-source/axis/devboard_lx/apps/osip" \
   CPP="gcc_cris -E -mlinux \
   -isystem  /ldata/axis/cris-source/axis/devboard_lx/os/linux/include" \
   LD="ld-cris -mcrisaout" AR="ar-cris" RANLIB="ranlib-cris" \
   NM="nm-cris" \
   ../osip/configure \
   --prefix=/ldata/axis/cris-source/axis/devboard_lx/target/cris-axis-linux-gnu/usr/local 

$> make

