#
# /etc/siproxd.conf - siproxd configuration file
#
# !! This is a sample file, adapt it to your needs before using it !!
#
# !! Strings MUST NOT contain spaces !!
#

######################################################################
# The interface names of INBOUND and OUTBOUND interface.
#
if_inbound  = eth0
if_outbound = ppp0


######################################################################
# Access control.
#    Access lists in the form: IP/mask (ex. 10.0.0.1/24)
#    Multiple entries may be separated by commas NO SPACES ARE ALLOWED!!
#    Empty list means 'does not apply' - no filtering is done then.
#    For *allow* lists this means: always allow, for *deny* lists that
#    this means never deny.
#
#    hosts_allow_reg: defines nets from which we accept registrations
#    hosts_allow_sip: defines nets from which we accept SIP traffic
#    hosts_deny_sip:  defines nets from which we deny SIP traffic
#
#    - The deny list takes precedence over the allow lists.
#    - The allow_reg list also implies allowance for sip.
#
#    Example for usage:
#      local private net -> allow_reg list
#      external nets (from which we accept incoming calls) -> allow_sip
#
#hosts_allow_reg = 192.168.1.8/24
#hosts_allow_sip = 123.45.0.0/16,123.46.0.0/16
#hosts_deny_sip  = 10.0.0.0/8,11.0.0.0/8


######################################################################
# Port to listen for incoming SIP messages.
#    5060 is usually the correct choice - don't change this unless you
#    know what you're doing
#
sip_listen_port = 5060


######################################################################
# Shall we daemonize?
#
daemonize = 1

######################################################################
# What shall I log to syslog?
#   0 - DEBUGs, INFOs, WARNINGs and ERRORs
#   1 - INFOs, WARNINGs and ERRORs (this is the default)
#   2 - WARNINGs and ERRORs
#   3 - only ERRORs
#   4 - absolutely nothing (be careful - you will have no way to
#                           see what siproxd is doing - or NOT doing)
silence_log = 1

######################################################################
# Shall I log call establishment to syslog?
#
log_calls = 1

######################################################################
# Secure Enviroment settings:
#   user:	uid/gid to switch to after startup
#   chrootjail:	path to chroot to (chroot jail)
user = nobody
#chrootjail = /var/lib/siproxd/

######################################################################
# Registration file:
#   Where to store the current registrations.
#   An empty value means we do not save registrations. Make sure that
#   the specified directory path does exist!
registration_file = /var/lib/siproxd/siproxd_registrations

######################################################################
# PID file:
#   Where to create the PID file.
#   This file holds the PID of the main thread of siproxd.
pid_file = /var/run/siproxd/siproxd.pid

######################################################################
# global switch to control the RTP proxy behaviour
#       0 - RTP proxy disabled
#       1 - RTP proxy (UDP relay of siproxd)
#
# Note: IPCHAINS and IPTABLES(netfilter) support is no longer present!
#    
rtp_proxy_enable = 1

######################################################################
# Port range to allocate listen ports from for incoming RTP traffic
#    This should be a range that is not blocked by the firewall
#    
rtp_port_low  = 7070
rtp_port_high = 7079

######################################################################
# Timeout for RTP streams
#    after this number of seconds, an RTP stream is considered dead
#    and proxying for it will be stopped.
#    Be aware that this timeout also applies to streams that are
#    in HOLD.
#    
rtp_timeout = 300

######################################################################
# Default Expiration timeout for Registrations
#    If a REGISTER request does not contain an Expires header
#    or expires= parameter in the Contact header, this number of
#    seconds will be used - and reported back to the UA in the answer.
#    
default_expires = 600

######################################################################
# Proxy authentication
#    If proxy_auth_realm is defined (a string), clients will be forced
#    to authenticate themselfes at the proxy (for registration only).
#    To disable Authentication, simply comment out this line.
#
#proxy_auth_realm = Authentication_Realm
#
# the (global) password to use (will be the same for all local clients)
#
#proxy_auth_passwd = password
#
# OR use individual per user passwords stored in a file
#
#proxy_auth_pwfile = /etc/siproxd_passwd.cfg
#
# 'proxy_auth_pwfile' has precedence over 'proxy_auth_passwd'

######################################################################
# Debug level... (setting to -1 will enable everything)
#
#  DBCLASS_BABBLE  0x00000001	   // babble (like entering/leaving func)
#  DBCLASS_NET     0x00000002	   // network
#  DBCLASS_SIP     0x00000004	   // SIP manipulations
#  DBCLASS_REG     0x00000008	   // Client registration
#  DBCLASS_NOSPEC  0x00000010	   // non specified class
#  DBCLASS_PROXY   0x00000020	   // proxy
#  DBCLASS_DNS     0x00000040	   // DNS stuff
#  DBCLASS_NETTRAF 0x00000080	   // network traffic
#  DBCLASS_CONFIG  0x00000100	   // configuration
#  DBCLASS_RTP     0x00000200      // RTP proxy
#  DBCLASS_ACCESS  0x00000400      // Access list evaluation
#  DBCLASS_AUTH    0x00000800      // Authentication
#
debug_level =      0x00000000

######################################################################
# TCP debug port
#
# You may connect to this port from a remote machine and
# receive the debug output. This allows bettwer creation of
# odebug output on embedded systems that do not have enough
# memory for large disk files.
# Port number 0 means this feature is disabled.
#
debug_port = 0

######################################################################
# Mask feature (experimental)
#
# Some UAs will always use the host/ip they register with as
# host part in the registration record (which will be the inbound
# ip address / hostname of the proxy) and can not be told to use a
# different host part in the registration record (like sipphone, FWD,
# iptel, ...)
# This Mask feature allows to force such a UA to be masqueraded to
# use different host.
# -> Siemens SIP Phones seem to need this feature.
#
# Unles you really KNOW that you need this, don't enable it.
#
# mask_host=<inbound_ip/hostname>
# masked_host=<hostname_to_be_masqueraded_as>
#
# mask_host=10.0.1.1			-- inbound IP address of proxy
# masked_host=my.public.host		-- outbound hostname proxy

######################################################################
# Outbound proxy
#
# Siproxd itself can be told to send all traffic to another
# outbound proxy.
# You can use this feature to 'chain' multiple siproxd proxies
# if you have several masquerading firewalls to cross.
#
# outbound_proxy_host = my.outboundproxy.org
# outbound_proxy_port = 5060

######################################################################
# Outbound proxy (Provider specific)
#
# Outbound proxies can be specified on a per-domain base.
# This allows to use an outbound proxy needed for ProviderA
# and none (or another) for ProviderB.
#
#outbound_domain_name = freenet.de
#outbound_domain_host = proxy.for.domain.freende.de
#outbound_domain_port = 5060
